**CD-1000 Single Pocket Discriminator**

  

**·** Single pocket Multi-currency Value counter with CF detection for USD, EUR and Local currencies  
**·** Up to 3 currencies can be installed. Easily open front head for easy maintenance

***Specifications***

* **· ECB Approved**
* **·** Sophisticated counterfeit note detection by UV, FL, MG, MT, IR
* **·** Value counting for USD, Euro and Local currency with full-size IR CIS
* **·** Program downloading through RS-232, USB port
* **·** 3.2” TFT Color LCD display
* **·** 4 direction (Face, Bottom, Width, Length) note recognition
* **·** Compact and attractive design
* **·** Option for 2-line external display or Dual screen display
* **·** Easily open front head for maintenance
* **·** Easy trouble-shoot by user from keypad
* **·** 3D size detection
* **·** Real Time Clock
* **·** Recording the counted result

|  |  |
| --- | --- |
| **MODEL** | **CD-1000** |
| **Optical Density Detection** | **O** |
| **Double (IR) Detection** | **O** |
| **Size Detection (For Height)** | **O** |
| **Size Detection (For Length) -3D** | **O** |
| **Ultraviolet (UV) & FL Detection** | **O** |
| **Magnetic (MG) Detection** | **O** |
| **Metal Thread (MT) Detection** | **O** |
| **Denomination Value Counting** | **O** |
| **Denomination Detection** | **Full sized IR CIS** |
| **Counting Speed, banknotes / minute** | **1000~1500** |
| **Display** | **3.2〃 TFT Color LCD** |
| **Hopper - Input Capacity, banknotes** | **300 (500)** |
| **Stacker - Output Tray Capacity, banknotes** | **200** |
| **Dimensions of Banknotes, mm** | **(m)50X100 / (M)90X180** |
| **Digit Display Capacity** | **9 digits** |
| **Batch Packaging Capacity, banknotes** | **Max. 999** |
| **Connectivity** | **Serial (RS-232) + USB** |
| **Power Consumption, W** | **AC100-240V, 50/60Hz** |
| **Dimensions, mm** | **270(w)X278(d)X257(h)** |
| **Net Weight, kg** | **7.3kg** |
| **Warranty, months** | **1 year** |